**SPERC factsheet – *Functional Fluids – Wide dispersive use (Solvent-borne)***

|  |  |
| --- | --- |
| **General Information** | |
| **Title of Specific ERC** | Functional Fluids (wide dispersive use): solvent-borne |
| **Applicable ERC** | 9a – Wide dispersive indoor use in closed systems; 9b – Wide dispersive outdoor use in closed systems |
| **Responsible** | ESIG/ESVOC |
| **Version** | V1 |
| **Code** | ESVOC 9.13b.v1  ESVOC 9.13c.v1 |
| **Scope** | Use as functional fluids e.g. cable oils, transfer oils, coolants, insulators, refrigerants, hydraulic fluids in professional equipment including maintenance and related material transfers and use of similar sealed items containing functional fluids for consumers.  *Substance Domain*: Applicable to petroleum substances (e.g., aliphatic and aromatic hydrocarbons) and petrochemicals (e.g., ketones, alcohols, acetates, glycols, glycol ethers, and glycol ether acetates).  *Size of installation*: Applicable to professional and consumer use with an assumed use rate of 0.05% of regional tonnage  *Processing conditions*: dry process |
| **Coverage** | Professional Uses (Process Categories): 1 (use in closed process, no likelihood of exposure), 2 (use in closed, continuous process with occasional controlled exposure), 3 (use in closed batch process (synthesis or formulation)), 8a (transfer of substance or preparation (charging/discharging) from/to vessels/large containers at non-dedicated facilities), 9  Transfer of substance or preparation into small containers (dedicated filling line, including weighing), 20 Heat and pressure transfer fluids in dispersive, professional use but closed systems.  Consumer Uses (Product Categories): 16 Heat transfer fluids, 17 Hydraulic fluids. |

|  |  |  |
| --- | --- | --- |
|  | **Characteristics of specific ERC** | **Type of Input Information** |
| **Operational Conditions** | Indoor use/outdoor use. Solvent-based process/product. Professional and consumer product use leading to emission of volatiles to air. Professional and consumer product use leading to disposal via the wastewater. |  |
| **Obligatory onsite RMMs** | No obligatory onsite RMMs assumed |  |
| **Substance Use Rate** | 0.05% (no geographical or temporal peaks in use) of Regional Tonnage based on default standard town population of 10000 inhabitants. | Default approach of the REACH guidance1 |
| **Days Emitting** | 365 days/year | Default approach of the REACH guidance1 |
| **Environmental Parameters for Fate Calculation** | Assumed dilution factor in freshwater is 10. For marine assessments an additional tenfold dilution is assumed, i.e., dilution factor in marine water = 100. | ERC default settings2 |

1ECHA Guidance on information requirements and chemical safety assessment, Chapter R.16: Environmental Exposure Estimation, Section R.16.3.2

2ECHA Guidance on information requirements and chemical safety assessment, Chapter R.16: Environmental Exposure Estimation, Section R.16.6.3

<http://echa.europa.eu/documents/10162/17224/information_requirements_r16_en.pdf>

|  |  |  |  |
| --- | --- | --- | --- |
|  | **Characteristics of Specific ERC** | | **Justification** |
| **Emission Fractions** | ***To Air*** | 0.05 | Average of ERC9a and 9b defaults3 |
| ***To Municipal Wastewater/Sewer/ Water courses*** | 0.025 | Average of ERC9a and 9b defaults3 |
| ***To Soil*** | 0.025 | Average of ERC9a and 9b defaults3 |

3ECHA Guidance on information requirements and chemical safety assessment, Chapter R.16: Environmental Exposure Estimation, Appendix R.16-1 Environmental Release Categories

|  |  |  |
| --- | --- | --- |
|  | **Type of RMM** | **Typical Efficiency** |
| **Appropriate Risk Management Measures (RMM) that may be used to achieve required emission reduction** | ***Air*** | |
| *Local/Onsite Technology* | Professional and Consumer product use with limited or no technical control of emission. |
| ***Water*** | |
| *Offsite Technology*  Municipal wastewater treatment plant | The removal efficiency of a sewage treatment plant can be estimated. The standard estimation is via the SimpleTreat module of EUSES or ECETOC TRA.  \*Specific substance efficiency calculated via SimpleTreat and is assumed to represent default removal efficiency. |
| *Local/Onsite Technology* | Professional and Consumer product use with limited or no technical control of emission. |

|  |
| --- |
| **Safe Use** |
| **Communication in SDS**  The REACH registrant establishes a set of standard conditions of safe use for a substance (for wide dispersive use of a solvent-borne processing aid) by adopting the conditions specified in this SPERC and recommending a Required Removal Efficiency (RRE) for adequate risk reduction. If RRE = 0, wastewater emission controls (beyond those specified by the operational conditions) are not required to ensure safe use of the substance. If > 0, the RRE may be achieved via offsite municipal sewage treatment (providing substance removal efficiency, REOffsite).  Removal efficiency requirements, as dictated by the assumed operating conditions, are documented in the Chemical Safety Report and communicated in the Safety Data Sheet. All other parameters underlying a substance exposure scenario based on the SPERC ‘Functional fluids – wide dispersive use (solvent-borne)’ are implicitly referred to via the reference to this SPERC.  **Scaling**  Not applicable for wide dispersive uses. |

### ESVOC 9.13.b-c.v1

|  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- |
| **Determinant Label** | **Quali-/ Quanti-tative** | **Value** | **Description of Value** | **Exposure route** | **Use conditions worker** | **Use condition consumer** | **Standard Phrase** |
| Indoor/Outdoor use | Qual | Covers Indoor and Outdoor use |  | Air/ water/ soil | e-w-3 | e-c-4 | Same as “value” |
|  |  |  |  |  |  |  |  |
|  |  |  |  |  |  |  |  |
|  |  |  |  |  |  |  |  |
|  |  |  |  |  |  |  |  |
|  |  |  |  |  |  |  |  |